# Adafruit BMP085 Library [![Build Status](https://github.com/adafruit/Adafruit-BMP085-Library/workflows/Arduino%20Library%20CI/badge.svg)](https://github.com/adafruit/Adafruit-BMP085-Library/actions)[![Documentation](https://github.com/adafruit/ci-arduino/blob/master/assets/doxygen_badge.svg)](http://adafruit.github.io/Adafruit-BMP085-Library/html/index.html)

This is a library for the Adafruit BMP085/BMP180 Barometric Pressure + Temp sensor

Designed specifically to work with the Adafruit BMP085 or BMP180 Breakout
  ----> http://www.adafruit.com/products/391
  ----> http://www.adafruit.com/products/1603

These displays use I2C to communicate, 2 pins are required to interface
Adafruit invests time and resources providing this open source code,
please support Adafruit and open-source hardware by purchasing
products from Adafruit!

Check out the links above for our tutorials and wiring diagrams

Requires the https://github.com/adafruit/Adafruit_BusIO library for I2C abstraction

Adafruit invests time and resources providing this open source code,
please support Adafruit and open-source hardware by purchasing
products from Adafruit!

Written by Limor Fried/Ladyada for Adafruit Industries.
BSD license, all text above must be included in any redistribution

To download. click the DOWNLOAD ZIP button, rename the uncompressed folder Adafruit_BMP085.
Check that the Adafruit_BMP085 folder contains Adafruit_BMP085.cpp and Adafruit_BMP085.h

Place the Adafruit_BMP085 library folder your arduinosketchfolder/libraries/ folder.
You may need to create the libraries subfolder if its your first library. Restart the IDE.

We also have a great tutorial on Arduino library installation at:
http://learn.adafruit.com/adafruit-all-about-arduino-libraries-install-use
