

		SSD1325		SSD1326		SSD1327		SSD1329
		128 x 80 x 4	256 x 32 x 4	128 x 128 x 4	128 x 128 x 4
	
0x15	set col		set col		set col		set col	
0x23	gr acc		-			-			-
0x24	draw rect		-			-			-
0x25	copy			-			-			-
0x26	scroll		scroll		scroll		-
0x27	-			-			scroll		-
0x2e	end move		end move		end move		-
0x2f		start move	start move	start move	-
0x75	set row		set row		set row		set row
0x81	contrast		contrast		contrast		contrast
0x82	-			-			-			2nd charge
0x84	current		current		nop			-
0x85	current		current		nop			-
0x86	current		current		nop			-
0x87	current		current		-

0x90	-			-			-			Icon ctl
0x91	-			-			-			Icon current
0x92	-			-			-			Icon current
0x93	-			-			-			Icon on/off
0x94	-			-			-			Icon all
0x95	-			-			-			Icon blink
0x96	-			-			-			Icon duty

0xa0	remap		remap		remap		remap
0xa1	start line		start line		start line		start line
0xa2	offset		offset		offset		offset
0xa4	mode		mode		mode		mode
..
0xa7	mode		mode		mode		mode
0xa8	multiplex ratio	multiplex ratio	multiplex ratio	multiplex ratio
0xab	-			-			regulator		-
0xad	master config	-			-			-
0xae		disp. on		disp. on		disp. on		disp. on
0xaf		disp. off		disp. off		disp. on		disp. on
0xb0	comp enable	-			-			-	
0xb1	phase len		phase len		phase len		phase len
0xb2	row period	frame freq	nop			frame freq
0xb3	div ratio [3]	clock div [2]	clock div 		clock div [2]	
0xb4	comp level	-			-			-
0xb5	-			-			GPIO			-
0xb6	-			-			2nd phase	-
0xb7	-			default gray	-			default gray
0xb8	gray level		gray level		gray level		gray level
0xb9	-			-			linear LUT		-
0xbb	-			2nd charge	nop			2nd charge
0xbc	precharge	precharge	precharge	precharge
0xbe	comh volt		comh volt		comh volt		comh volt
0xbf		VSL			-			-			-
0xd5	-			-			fn select B	-
0xe3	nop			-			-			nop
0xfd		-			cmd lock		cmd lock		cmd lock

