# plu.bex
# 
# switches are at PIO0_10 and PIO0_2
# Because only PIO0_10 or PIO0_2 can be used as input for PLU,
# PIO0_10 is routed via LVLSHFT0 path to PIO0_22

PIO0_22 <= LVLSHFT_OUT0; 

LVLSHFT_IN0 <= PIO0_10; 

#PIO0_9 <= !PIO0_2 & !PIO0_22; 

PLU_CLKIN <= CLKOUT;
