<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<text>D4</text>
<text>D2</text>
<text>D1</text>
<text>RX</text>
<text>TX</text>
<text>D3</text>
<text>G</text>
<text>RST</text>
<text>5V</text>
<text>D5</text>
<text>D6</text>
<text>A0</text>
<text>3V3</text>
<text>D8</text>
<text>D7</text>
<text>D0</text>
<wire x1="25.4" y1="31.75" x2="25.4" y2="1.27" width="0.0254" layer="20"/>
<wire x1="24.13" y1="0" x2="3.175" y2="0" width="0.0254" layer="20"/>
<wire x1="0" y1="7.62" x2="0" y2="31.75" width="0.0254" layer="20"/>
<wire x1="0" y1="31.75" x2="1.27" y2="33.02" width="0.0254" layer="20" curve="-90"/>
<wire x1="1.27" y1="33.02" x2="24.13" y2="33.02" width="0.0254" layer="20"/>
<wire x1="24.13" y1="33.02" x2="25.4" y2="31.75" width="0.0254" layer="20" curve="-90"/>
<wire x1="25.4" y1="1.27" x2="24.13" y2="0" width="0.0254" layer="20" curve="-90"/>
<wire x1="0" y1="7.62" x2="1.905" y2="6.35" width="0.0254" layer="20"/>
<wire x1="1.905" y1="6.35" x2="1.905" y2="1.27" width="0.0254" layer="20"/>
<wire x1="1.905" y1="1.27" x2="3.175" y2="0" width="0.0254" layer="20" curve="90"/>
<text>2.1mm</text>
<text>7-14Vdc</text>
<text>+</text>
<text>+</text>
<text>D1 Mini Power Shield</text>
<text>by Jon Oxer</text>
<text>(C)2016 SuperHouse
Automation Pty Ltd</text>
<text>superhouse.tv/d1mpower</text>
<text>Output 5V 800mA</text>
<text>Input 7-14Vdc</text>
<text>INPUT</text>
<text>v1.0</text>
<text>A</text>
<text>C</text>
<text>C</text>
<text>A</text>
</plain>
<libraries>
<library name="freetronics-original">
<description>Spark Fun Electronics' preferred foot prints. We've spent an enormous amount of time creating and checking these footprints and parts.
If you enjoy using this library, please buy one of our products at http://www.sparkfun.com.
Please also note that we guarantee that there are some messed up footprints in this library.
We've tried to note which are proven and tested but by downloading this file, you acknowledge that you are using this file at your own risk.
We cannot be held responsible for faulty PCBs. Always check your parts against a 1:1 printout.

Licensing: CC v3.0 Share-Alike You are welcome to use this library for commercial purposes.
For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold.
We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
</packages>
</library>
<library name="freetronics">
<packages>
<package name="POWER_JACK_PTH">
</package>
<package name="SMB-DIODE">
<description>&lt;b&gt;Diode&lt;/b&gt;&lt;p&gt;
Basic small signal diode good up to 200mA. SMB footprint. Common part #: BAS16</description>
</package>
<package name="0603">
</package>
</packages>
</library>
<library name="linear">
<packages>
<package name="DPACK">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;
(Motorola)</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="PANASONIC_D">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="freetronics-jon">
<packages>
<package name="LED-0603">
</package>
<package name="0603">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="H1" library="freetronics-original" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="H2" library="freetronics-original" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="freetronics" package="POWER_JACK_PTH" value="DC_2_1MM"/>
<element name="IC1" library="linear" package="DPACK" value="MC33269DT-5.0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="PANASONIC_D" value="47uF 25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="PANASONIC_D" value="47uF 25V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="freetronics" package="SMB-DIODE" value="1N4004 SMB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="freetronics" package="0603" value="100nF 0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="freetronics-jon" package="LED-0603" value="BLUE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="freetronics-jon" package="0603" value="2K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="freetronics-jon" package="SCREWTERMINAL-3.5MM-2" value=""/>
</elements>
<signals>
<signal name="S$2">
</signal>
<signal name="GND">
<contactref element="H2" pad="7"/>
<contactref element="C1" pad="-"/>
<contactref element="J2" pad="GNDBREAK"/>
<contactref element="J2" pad="GND"/>
<contactref element="IC1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="-"/>
<contactref element="LED1" pad="C"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="D1">
<contactref element="H2" pad="3"/>
</signal>
<signal name="D2">
<contactref element="H2" pad="4"/>
</signal>
<signal name="D5">
<contactref element="H1" pad="4"/>
</signal>
<signal name="D6">
<contactref element="H1" pad="5"/>
</signal>
<signal name="D7">
<contactref element="H1" pad="6"/>
</signal>
<signal name="D8">
<contactref element="H1" pad="7"/>
</signal>
<signal name="A0">
<contactref element="H1" pad="2"/>
</signal>
<signal name="D0">
<contactref element="H1" pad="3"/>
</signal>
<signal name="D3">
<contactref element="H2" pad="5"/>
</signal>
<signal name="D4">
<contactref element="H2" pad="6"/>
</signal>
<signal name="RX">
<contactref element="H2" pad="2"/>
</signal>
<signal name="TX">
<contactref element="H2" pad="1"/>
</signal>
<signal name="5V">
<contactref element="H2" pad="8"/>
<contactref element="C3" pad="+"/>
<contactref element="IC1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="RST">
<contactref element="H1" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="H1" pad="8"/>
</signal>
<signal name="VIN">
<contactref element="D1" pad="C"/>
<contactref element="IC1" pad="3"/>
<contactref element="C1" pad="+"/>
</signal>
<signal name="N$8">
<contactref element="J2" pad="PWR"/>
<contactref element="D1" pad="A"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
